{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Munka1","Munka2","Munka3"],"not_rendered":{"charts":4,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Munka1","index":0,"n_rows":12,"n_cols":12,"rows_kept":12,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["frekvencia","U, Ueff","I (microA)","R, Z",{"$nulls":6},0,0.11627906976744186]
[0,5,43,0.11627906976744186,"DC",null,0,0.11627906976744186,null,null,1.2041199826559246,0.23566666666666664]
[16,3.5349999999999997,15,0.23566666666666664,"AC",null,16,0.23566666666666664,null,null,1.5051499783199058,0.04700797872340425]
[32,3.5349999999999997,75.2,0.04700797872340425,"AC",null,32,0.04700797872340425,null,null,1.8061799739838869,0.03178956834532374]
[64,3.5349999999999997,111.2,0.03178956834532374,"AC",null,64,0.03178956834532374,null,null,2.0969100130080562,0.02067251461988304]
[125,3.5349999999999997,171,0.02067251461988304,"AC",null,125,0.02067251461988304,null,null,2.397940008672037,0.012761732851985558]
[250,3.5349999999999997,277,0.012761732851985558,"AC",null,250,0.012761732851985558,null,null,2.6989700043360183,0.008240093240093239]
[500,3.5349999999999997,429,0.008240093240093239,"AC",null,500,0.008240093240093239,null,null,2.9999999999999996,0.005480620155038759]
[1000,3.5349999999999997,645,0.005480620155038759,"AC",null,1000,0.005480620155038759,null,null,3.301029995663981,0.003588832487309644]
[2000,3.5349999999999997,985,0.003588832487309644,"AC",null,2000,0.003588832487309644,null,null,3.602059991327962,0.0021554878048780485]
[4000,3.5349999999999997,1640,0.0021554878048780485,"AC",null,4000,0.0021554878048780485,null,null,3.9030899869919433,0.001309]
[8000,3.5349999999999997,2700,0.0013092592592592591,"AC",null,8000,0.0013092592592592591]

{"sheet":"Munka2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Munka3","index":2,"n_rows":46,"n_cols":7,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["A mérés menete"]
[]
["egyenáram: DC-ellenállás, f=0, Ugen1=5V*Ucoarse*Ufine=5V",{"$nulls":5},"R=Ugen/Ibőr"]
["impedancia: AC-ellenállás 16Hz<f<8000Hz Ugen;eff=Ugen1*",{"$nulls":4},"gen1*gyök2/2"]
[{"$nulls":6},"Z=Ug;eff/Ibőr;eff"]
[]
["f","U","I(µA)","R, Z"]
[0,5,30,0.16666666666666666,"DC"]
[16,3.5349999999999997,35.3,0.10014164305949008,"AC"]
[32,3.5349999999999997,39.8,0.08881909547738694]
[64,3.5349999999999997,49.5,0.0714141414141414]
[125,3.5349999999999997,70.2,0.05035612535612535]
[250,3.5349999999999997,109.7,0.032224247948951686]
[500,3.5349999999999997,156.2,0.02263124199743918]
[1000,3.5349999999999997,405,0.008728395061728395]
[2000,3.5349999999999997,676,0.005229289940828402]
[4000,3.5349999999999997,1168,0.003026541095890411]
[8000,3.5349999999999997,1975,0.0017898734177215188]
{"$rows_empty":19}
["fajlagos ellenállás:"]
["ρ*=R*A",null,0.00020514666666666669,"kOhm*m2"]
["d=14mm=0,014m"]
[0.0012308800000000002]
[]
["fajlagos kapacitás:"]
["Ɣ*=C/A",null,14.822105617703357,"kF/m2"]
["C=1/(2πfZ)"]
[0.01824423336271871]